{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Summary","Power - Abs","Power - Hyd","Power - Hyd ROi","Flow - Pump out","Flow - Perm","Flow - RO pre","Flow - RO post","Pressure - RO"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Tab Name ","Description ","Units"]
[null,"Summary ","Summary table describing which tab cooresponds to which WEC-Sim output matrix"," - "]
[null,"Power - Abs","The average absorbed power from the WEC (calculated from anchor reaction force and heave velocity) ","Watts"]
[null,"Power - Hyd","The average hydraulic power output at pump (calculated from pump output flow and pressure)","Watts"]
[null,"Power - Hyd Roi","The average hydraulic power measured at the RO system inlet (calculated from RO system pressure and flow (pre-accumulator))","Watts"]
[null,"Flow - Pump out","The average flowrate measured at the pump outlet","GPM"]
[null,"Flow - Perm","The average permeate (clean water) production ","GPM"]
[null,"Flow - RO (pre)","The average flowrate measured at the inlet of the RO system before the accumulators","GPM"]
[null,"Flow - RO (post)","The average flowrate measured after the accumulator bank in the RO system","GPM"]
[null,"Pressure - RO","The average pressure measured at the inlet of the RO system ","PSI"]

{"sheet":"Power - Abs","index":1,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[3,0,17,0],[1,2,1,10]]}
["Absorbed Power - Watts"]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,16.484999999999999,15.114000000000001,13.727,12.044,10.688000000000001,9.3202999999999996,9.17,7.8129,7.3947000000000003]
[null,0.5,99.555000000000007,89.146000000000001,81.578000000000003,70.704999999999998,62.356000000000002,58.790999999999997,53.204000000000001,46.411000000000001,42.451999999999998]
[null,0.75,259.73,214.35,192.94,181.69,162.59,149.16,136.85,115.54,109.79]
[null,1,458.89,403.36,361.06,323.35000000000002,284.41000000000003,266.35000000000002,243.2,212.07,194.41]
[null,1.25,694.97,619.36,533.54999999999995,496.73,430.95,387.98,352.91,306.20999999999998,289.20999999999998]
[null,1.5,0,844.9,718.99,638.25,570.09,508.57,465.96,420.08,384.76]
[null,1.75,0,0,925.16,828.56,736.64,668.56,603.91,536.75,491.06]
[null,2,0,0,0,1025.4000000000001,904.97,808.08,740.03,633.14,602.17999999999995]
[null,2.25,0,0,0,0,1108.7,966.53,877.22,778.68,723.52]
[null,2.5,0,0,0,0,0,1119.5999999999999,1036.7,917.29,823.23]
[null,2.75,0,0,0,0,0,0,1158.5,1059.2,932.34]
[null,3,0,0,0,0,0,0,0,1175.8,1059.5999999999999]
[null,3.25,0,0,0,0,0,0,0,1342,1202.3]
[null,3.5,0,0,0,0,0,0,0,0,1354.8]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Power - Hyd","index":2,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Hydraulic Power at pump outlet - Watts"]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,9.6259999999999994,8.9292999999999996,8.2972999999999999,7.4057000000000004,6.6318000000000001,5.7862,5.8068,4.9458000000000002,4.7205000000000004]
[null,0.5,53.322000000000003,49.404000000000003,45.930999999999997,41.006,37.023000000000003,35.396999999999998,32.616,28.824000000000002,26.486000000000001]
[null,0.75,123.14,107.75,100.69,97.569000000000003,89.38,83.914000000000001,78.724999999999994,67.69,64.932000000000002]
[null,1,195.18,181.87,171.07,159.01,145.58000000000001,139.16,130.56,116.56,108.27]
[null,1.25,268.95,253.62,230.33,223.31,202.71,187.28,176.31,158.47,152.41999999999999]
[null,1.5,0,319.64999999999998,288.64,266.08999999999997,248.95,229.28,218.91,203.43,190.59]
[null,1.75,0,0,344.03,321.45999999999998,300.01,280.92,263.52,243.77,229.49]
[null,2,0,0,0,373.46,347.33,321.31,302.95,271.32,263.94]
[null,2.25,0,0,0,0,400.95,363.78,341.46,313.41000000000003,300.47000000000003]
[null,2.5,0,0,0,0,0,402.34,383.69,352.35,325.37]
[null,2.75,0,0,0,0,0,0,412.36,388.25,354.8]
[null,3,0,0,0,0,0,0,0,415.87,387]
[null,3.25,0,0,0,0,0,0,0,461.42,424.34]
[null,3.5,0,0,0,0,0,0,0,0,462.53]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Power - Hyd ROi","index":3,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Hydraulic Power at RO inlet - Watts"]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,7.5622999999999996,6.9336000000000002,6.4337999999999997,5.702,5.0796999999999999,4.3906000000000001,4.4298999999999999,3.7566000000000002,3.569]
[null,0.5,29.931999999999999,28.965,27.634,26.286000000000001,25.073,24.396999999999998,23.288,21.527000000000001,20.129000000000001]
[null,0.75,39.442999999999998,38.18,37.625,37.411999999999999,36.491999999999997,35.58,34.926000000000002,33.009,32.518000000000001]
[null,1,46.066000000000003,45.625999999999998,44.786999999999999,44.51,43.235999999999997,42.542000000000002,41.872,40.447000000000003,39.4]
[null,1.25,52.109000000000002,51.645000000000003,50.098999999999997,50.462000000000003,48.978999999999999,47.774000000000001,46.978000000000002,45.244,44.811999999999998]
[null,1.5,0,57.064999999999998,55.128999999999998,54.234999999999999,53.268000000000001,51.87,51.23,50.003,48.865000000000002]
[null,1.75,0,0,60.048000000000002,59.119,57.603000000000002,56.601999999999997,55.692999999999998,53.817,52.914000000000001]
[null,2,0,0,0,63.747,61.793999999999997,60.432000000000002,59.43,56.643999999999998,56.212000000000003]
[null,2.25,0,0,0,0,66.807000000000002,64.375,63.134,60.848999999999997,59.784999999999997]
[null,2.5,0,0,0,0,0,67.983999999999995,66.926000000000002,64.415000000000006,62.097000000000001]
[null,2.75,0,0,0,0,0,0,69.983000000000004,67.954999999999998,65.114999999999995]
[null,3,0,0,0,0,0,0,0,70.835999999999999,68.253]
[null,3.25,0,0,0,0,0,0,0,75.173000000000002,72.125]
[null,3.5,0,0,0,0,0,0,0,0,76.33]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Flow - Pump out","index":4,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Flowrate at pump outlet - Gallons/minute "]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,0.29807,0.28410999999999997,0.26602999999999999,0.24364,0.2233,0.19943,0.19889999999999999,0.17474000000000001,0.16855999999999999]
[null,0.5,1.2017,1.1343000000000001,1.0643,0.96723999999999999,0.89031000000000005,0.85023000000000004,0.79896999999999996,0.72060000000000002,0.67090000000000005]
[null,0.75,2.5124,2.2313000000000001,2.0985999999999998,2.0409000000000002,1.8894,1.7777000000000001,1.6845000000000001,1.4716,1.4178999999999999]
[null,1,3.7942,3.5526,3.3601000000000001,3.1575000000000002,2.9047999999999998,2.7766000000000002,2.6248,2.3721999999999999,2.2136]
[null,1.25,5.0087000000000002,4.7548000000000004,4.3617999999999997,4.2470999999999997,3.8902999999999999,3.5960000000000001,3.4106999999999998,3.1040000000000001,2.9981]
[null,1.5,0,5.7812999999999999,5.2915000000000001,4.9272999999999998,4.6364999999999998,4.2877000000000001,4.1273,3.8561000000000001,3.6349999999999998]
[null,1.75,0,0,6.1136999999999997,5.7668999999999997,5.4432,5.1098999999999997,4.8350999999999997,4.5118999999999998,4.2766000000000002]
[null,2,0,0,0,6.5073999999999996,6.1345999999999998,5.7268999999999997,5.4192,4.9291999999999998,4.8044000000000002]
[null,2.25,0,0,0,0,6.8621999999999996,6.3358999999999996,5.9821999999999997,5.5575000000000001,5.3575999999999997]
[null,2.5,0,0,0,0,0,6.8414000000000001,6.5861000000000001,6.1208999999999998,5.7037000000000004]
[null,2.75,0,0,0,0,0,0,6.9341999999999997,6.6045999999999996,6.1249000000000002]
[null,3,0,0,0,0,0,0,0,6.9503000000000004,6.5465]
[null,3.25,0,0,0,0,0,0,0,7.5555000000000003,7.0301]
[null,3.5,0,0,0,0,0,0,0,0,7.4871999999999996]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Flow - Perm","index":5,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Permeate flowrate (clean water production) - Gallons/minute "]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,1.9938999999999998E-2,1.8071E-2,1.6853E-2,1.4539E-2,1.2683E-2,1.0644000000000001E-2,1.0544E-2,8.6952000000000002E-3,7.9631000000000007E-3]
[null,0.5,7.0069999999999993E-2,6.7215999999999998E-2,6.4856999999999998E-2,6.2687999999999994E-2,6.0007999999999999E-2,5.8625999999999998E-2,5.5969999999999999E-2,5.2658000000000003E-2,4.9893E-2]
[null,0.75,8.7247000000000005E-2,8.4708000000000006E-2,8.3506999999999998E-2,8.2960999999999993E-2,8.1087000000000006E-2,7.9230999999999996E-2,7.7785999999999994E-2,7.4559E-2,7.3748999999999995E-2]
[null,1,9.8066E-2,9.6889000000000003E-2,9.5843999999999999E-2,9.4291E-2,9.2619000000000007E-2,9.1204999999999994E-2,8.9817999999999995E-2,8.7626999999999997E-2,8.5862999999999995E-2]
[null,1.25,0.1074,0.10634,0.10425,0.10366,0.10161000000000001,9.9695000000000006E-2,9.8123000000000002E-2,9.5576999999999995E-2,9.4855999999999996E-2]
[null,1.5,0,0.11441999999999999,0.11171,0.10961,0.1082,0.1061,0.10484,0.10316,0.1013]
[null,1.75,0,0,0.11838,0.11652,0.11462,0.113,0.11146,0.10913,0.10739]
[null,2,0,0,0,0.12307,0.12056,0.11834,0.11686000000000001,0.11327,0.11252]
[null,2.25,0,0,0,0,0.12715000000000001,0.12376,0.12205000000000001,0.11884,0.11772000000000001]
[null,2.5,0,0,0,0,0,0.12839,0.12701999999999999,0.12371,0.12089999999999999]
[null,2.75,0,0,0,0,0,0,0.13097,0.12837000000000001,0.12503]
[null,3,0,0,0,0,0,0,0,0.13197999999999999,0.12891]
[null,3.25,0,0,0,0,0,0,0,0.13749,0.13372999999999999]
[null,3.5,0,0,0,0,0,0,0,0,0.13875000000000001]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Flow - RO pre","index":6,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Flowrate at RO system inlet (pre-accumulators) - Gallons/minute "]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,0.29807,0.28410999999999997,0.26602999999999999,0.24364,0.2233,0.19943,0.19889999999999999,0.17474000000000001,0.16855999999999999]
[null,0.5,0.84828999999999999,0.84421000000000002,0.81132000000000004,0.78293999999999997,0.75924999999999998,0.73782999999999999,0.71664000000000005,0.67361000000000004,0.63934000000000002]
[null,0.75,1.0204,1.0023,0.99519999999999997,0.99719000000000002,0.98421999999999998,0.96104999999999996,0.95433000000000001,0.91281999999999996,0.90359]
[null,1,1.1336999999999999,1.1295999999999999,1.1126,1.1261000000000001,1.0973999999999999,1.0827,1.0734999999999999,1.0474000000000001,1.0290999999999999]
[null,1.25,1.2298,1.2253000000000001,1.1990000000000001,1.2181999999999999,1.1930000000000001,1.1665000000000001,1.1569,1.127,1.1227]
[null,1.5,0,1.3071999999999999,1.2774000000000001,1.2742,1.2574000000000001,1.2309000000000001,1.2244999999999999,1.2034,1.1874]
[null,1.75,0,0,1.3531,1.347,1.3212999999999999,1.304,1.2937000000000001,1.2611000000000001,1.2524]
[null,2,0,0,0,1.4118999999999999,1.3811,1.3629,1.3478000000000001,1.3043,1.2992999999999999]
[null,2.25,0,0,0,0,1.4525999999999999,1.4204000000000001,1.4014,1.3696999999999999,1.3515999999999999]
[null,2.5,0,0,0,0,0,1.4715,1.4558,1.42,1.3836999999999999]
[null,2.75,0,0,0,0,0,0,1.4977,1.4696,1.4277]
[null,3,0,0,0,0,0,0,0,1.5101,1.4731000000000001]
[null,3.25,0,0,0,0,0,0,0,1.5691999999999999,1.5267999999999999]
[null,3.5,0,0,0,0,0,0,0,0,1.5827]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Flow - RO post","index":7,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Flowrate at RO  inlet (post-accumulators) - Gallons/minute "]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,0.22631000000000001,0.20510999999999999,0.19128999999999999,0.16502,0.14394999999999999,0.1208,0.11967,9.8691000000000001E-2,9.0382000000000004E-2]
[null,0.5,0.79529000000000005,0.76290999999999998,0.73612999999999995,0.71150999999999998,0.68108999999999997,0.66539999999999999,0.63526000000000005,0.59767000000000003,0.56628000000000001]
[null,0.75,0.99026000000000003,0.96143000000000001,0.94779999999999998,0.94160999999999995,0.92034000000000005,0.89927999999999997,0.88287000000000004,0.84624999999999995,0.83704999999999996]
[null,1,1.1131,1.0996999999999999,1.0878000000000001,1.0702,1.0511999999999999,1.0351999999999999,1.0194000000000001,0.99456,0.97453999999999996]
[null,1.25,1.2190000000000001,1.2070000000000001,1.1832,1.1765000000000001,1.1533,1.1315,1.1136999999999999,1.0848,1.0766]
[null,1.5,0,1.2986,1.2679,1.2441,1.228,1.2042999999999999,1.1899,1.1709000000000001,1.1497999999999999]
[null,1.75,0,0,1.3435999999999999,1.3225,1.3008999999999999,1.2826,1.2650999999999999,1.2385999999999999,1.2188000000000001]
[null,2,0,0,0,1.3968,1.3683000000000001,1.3431999999999999,1.3263,1.2856000000000001,1.2770999999999999]
[null,2.25,0,0,0,0,1.4431,1.4047000000000001,1.3853,1.3488,1.3361000000000001]
[null,2.5,0,0,0,0,0,1.4572000000000001,1.4417,1.4040999999999999,1.3723000000000001]
[null,2.75,0,0,0,0,0,0,1.4865999999999999,1.4570000000000001,1.4191]
[null,3,0,0,0,0,0,0,0,1.4979,1.4631000000000001]
[null,3.25,0,0,0,0,0,0,0,1.5606,1.5179]
[null,3.5,0,0,0,0,0,0,0,0,1.5748]
[null,3.75,0,0,0,0,0,0,0,0,0]

{"sheet":"Pressure - RO","index":8,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,2,1,10],[3,0,17,0]]}
["Pressure at RO system inlet - pounds/square inch"]
[null,null,"Period [sec]"]
[null,null,5,6,7,8,9,10,11,12,13]
["Signficant Wave Height [m]",0.25,60.521999999999998,60.302,59.351999999999997,57.945,56.884999999999998,55.796999999999997,55.287999999999997,54.442,54.192]
[null,0.5,82.03,80.7,79.674999999999997,78.811000000000007,77.632000000000005,76.986000000000004,75.798000000000002,74.376999999999995,73.311999999999998]
[null,0.75,88.912000000000006,87.885000000000005,87.378,87.153000000000006,86.326999999999998,85.56,84.894000000000005,83.57,83.230999999999995]
[null,1,93.224999999999994,92.756,92.338999999999999,91.694000000000003,91.022000000000006,90.424000000000007,89.882000000000005,88.986999999999995,88.266000000000005]
[null,1.25,96.947000000000003,96.525000000000006,95.69,95.450999999999993,94.635000000000005,93.873999999999995,93.245999999999995,92.215999999999994,91.923000000000002]
[null,1.5,0,99.744,98.664000000000001,97.826999999999998,97.263999999999996,96.43,95.924000000000007,95.256,94.509]
[null,1.75,0,0,101.32,100.58,99.822999999999993,99.18,98.563999999999993,97.635999999999996,96.941000000000003]
[null,2,0,0,0,103.19,102.19,101.31,100.72,99.287000000000006,98.986000000000004]
[null,2.25,0,0,0,0,104.82,103.47,102.79,101.51,101.06]
[null,2.5,0,0,0,0,0,105.31,104.77,103.45,102.33]
[null,2.75,0,0,0,0,0,0,106.34,105.31,103.97]
[null,3,0,0,0,0,0,0,0,106.74,105.52]
[null,3.25,0,0,0,0,0,0,0,108.94,107.44]
[null,3.5,0,0,0,0,0,0,0,0,109.45]
[null,3.75,0,0,0,0,0,0,0,0,0]